Special Customer Requirement

#### *( Production and Shipping requirements )*

**#432**

# Customer(s):

**TECH GRADE**

**Product: C1T2250GI** *( TSS-2250 )*

**- Tech Grade** - USP Grade - Liquid

* Screened 20/60 **- Screened 60** - Other

#### ( *screen out dust* )

* Take Samples -

# Production / Packaging:

Type of Film - Weight per Bag

Number of Bags per pallet Pallet

*1*

Configuration

### *Must be centered on pallet*

Type of Sacks - **Weight per Bag *2,250-lbs***

|  |  |  |
| --- | --- | --- |
| - Shrink Wrap - | - Date, Time & Lot # on each Bag | - Number and Initial each pallet |
| - Liners Required - | - Heat Treated Pallets | - Super sack Tags |

# Shipping:

* Placards or Tags Required - *Must have 1 Super Sack Tag attached to a Sack Strap.*
* Stickers Required -
* Other Requirements - *Must have placards stating “TSS-2250”*

### General - *Load according to Giles loading chart and quantity on Bill of Lading*

*Container must have block and bracing around load before shipping*

* Air Bags **- Double Wrap - Corner Boards - Block & Brace**
* Must have Quality Approval before loading - Must have Management Approval before loading

**- Other -**

CoA with each shipment. CoA with BOL.

Show PO# and SAP#(109931) on CoA.

**Revision History:**

|  |  |
| --- | --- |
| Date | Change |
| *04/10/15* | *New SCR* |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

*Date Printed - 4/14/15*