Special Customer Requirement

*(Production and Shipping Requirements)*

**#120**

**Customer(s):**

|  |  |
| --- | --- |
| **Abbott Laboratories**  16th St. & Sheridan rd.  BLDG. S16  N. Chicago, IL 60064 | **\*\*\*Heat Treated Pallets\*\*\*** |

**Product: T50- H&F Abbvie**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **- Tech Grade** | | - USP Grade | - Liquid: |  |
| - Screened 20/60 | | - **Screened 60** | - Other: |  |
|  | | (Screen Out Dust) |  |  |
| - Take Samples - |  | | | |

**Production / Packaging:**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Type of Film: | ***Giles Tech 50-lb Film*** | | | | | | | | Weight per Bag: | ***50 lbs*** |
| Number of Bags per Pallet: | | | | ***49*** | | Pallet Configuration: | ***7 per layer x 7 layers*** | | | |
| Type of Sacks: |  | | | | | | | | Weight per Sack: |  |
| **- Shrink Wrap** | | | **- Date, Time & Lot # on each Bag** | | | | | **- Number and Initial each pallet** | | |
| - Liners Required | | | - Bottom Tie Grommets | | | | | - Super Sack Tags | | |
| **- Placards or Tags Required:** | | | | | ***A placard with PO# and code – 27740 on each pallet*** | | | | | |
| - Stickers Required: | |  | | | | | | | | |
| **- Other Requirements:** | | | | ***Use printer code 6 - #27740 must be on each bag*** | | | | | | |
| **- Other Requirements:** | | | | ***Must be on HARDWOOD HEAT TREATED PALLETS*** | | | | | | |

**Shipping:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **- General:** | | ***Load according to Giles loading chart and quantity on Bill of Lading*** | | | | |
| - Air Bags | | | - Double Wrap | - Corner Boards | - |  |
| - Must have Quality Approval before loading | | | | - Must have Management Approval before loading | | |
| **- Other:** | ***The expiration date must be WRITTEN IN on the COA*** | | | | | |

**Revision History:**

|  |  |
| --- | --- |
| **Date** | **Change** |
| 05/03/06 | New SCR (Replacing SCR #1) |
| 04/28/10 | Added “ Must be on HARDWOOD HEAT TREATED PALLETS” |
| 11/03/14 | Marked Screened 60 |
|  |  |
|  |  |
|  |  |