**Quiz**

1. What is the proper sequence of listing the basic description on shipping papers?

A. **I**dentification Number, Proper **S**hipping Name, **H**azard Class,**P**ackaging Group

B. Proper **S**hipping Name, **H**azard Class, **I**dentification Number, **P**ackaging Group

C. **P**ackaging Group, **I**dentification Number, **H**azard Class

D. None of the above

2. The person providing the hazardous material shipping papers must maintain a copy for:

A. The duration of the shipment.

B. For one month.

C. For one year.

D. For two years.

3. The Identification Number for Sulfuric Acid is:

A. 1812

B. 1492

C. 1950

D. 1830

4. In the Hazardous Materials Table, PG (packing group) is an indication of:

A. The size of the hazmat packaging

B. The weight of the hazmat packaging

C. The degree of danger the material presents

D. The size and the weight of the hazmat packaging

5. Sulfuric acid is a corrosive. The proper hazard class is:

A. 3

B. 4

C. 1

D. 8

6. The proper entry of a hazardous material on a shipping paper must show:

A. The name of the shipper, the basic description of the material, ID number

B. Only the description

C. Only the shipping name and ID number

D. Description and emergency response phone number (if required)

7. Placards must be placed:

A. On each side and each end of the hazardous material package

B. On each side and each end of the transport vehicle or railcar

C. On the top of the hazardous material package

D. On the rear of the transport vehicle

8. The emergency response telephone number listed on the shipping papers:

A. can be an answering machine.

B. must be monitored at all times while the material in is transit.

C. is only necessary while the materials are being loaded or unloaded.

D. is not required.

9. Hazardous material warning labels List:

A. The contents, weight, and destination of the hazmat package

B. The description, weight and destination of the hazmat package

C. The correct class and division of hazard of the hazmat package

D. Warning labels are color-coded only

10. Proper shipping names appear in the Hazardous Materials Table as:

A. Highlighted

B. Italic print

C. All CAPITALS

D. Roman type

Name / Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Trainer: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_