Special Customer Requirement

*( Production and Shipping requirements )*

**#429**

**Customer(s):**

**General Tech Grade**



**Super Sacks For Magriculture**

**Product: TSS with Magriculture Placards**

|  |  |  |  |
| --- | --- | --- | --- |
| **- Tech Grade** | - USP Grade | - Liquid |  |
| - Screened 20/60 | - Screened 60 | - Other |  |
|  | ( *screen out dust* ) |  |  |

- Take Samples -

**Production / Packaging:**

Type of Film - Weight per Bag

Number of Bags per pallet *1* Pallet Configuration *Must be centered on pallet*

Type of Sacks - *Stencil sacks with” 2,000” lb stencil* Weight per Bag *2,000-lbs*

|  |  |  |
| --- | --- | --- |
| - Shrink Wrap - | - Date, Time & Lot # on each Bag | - Number and Initial each pallet |
| - Liners Required - | - Bottom Tie Grommets | - Super sack Tags |

**- Tags Required -** *Must have 1 Super Sack Tag attached to a Sack Strap*

**- Placards Required -** *Must have 1 Magriculture placard in color – placed in the*

*plastic pouch on the front of each super sack*

**- Other Requirements -**  *"TSS" is to be written on the back of Super Sack Tag*

**Shipping:**

- **General** -  *Load according to Giles loading chart and quantity on Bill of Lading*

- Air Bags - Double Wrap - Corner Boards -

- Must have Quality Approval before loading - Must have Management Approval before loading

- **Other** - **Must Line the sides, front of trailer and between sacks with card board**

**Revision History:**

|  |  |
| --- | --- |
| Date | Change |
| *05/06/13* | *New SCR -* |
|  |  |
|  |  |
|  |  |

*Date Printed - 10/07/13*