**Quiz**

|  |  |  |  |
| --- | --- | --- | --- |
| 1. | True | False | Hazardous Materials are those materials that burn, explode, or react violently or that can cause harm to people, property or environment. |
| 2. | True | False | The hazardous material warning label identifies the weight and contents of the package |
| 3. | True | False | DOT regulations define only 4 hazard classifications for Hazardous Materials. |
| 4. | True | False | The Packing Group indicates the relative degree of danger of the material. The Packing Group III represents the GREATEST DANGER |
| 5. | True | False | If “NA” appears in the identification number that means it’s Not Applicable |
| 6. | True | False | Hazmat Employees are ones who directly affects the safe transportation of hazardous materials, either as a self-employed person or one who performs duties relating to hazardous materials as part of the job. |
| 7. | True | False | Labels and placards communicate important information to emergency responders in the event of an incident |
| 8. | True | False | Hazard labels and placards are square or oval shaped |
| 9. | True | False | Hazard labels convey information by using color, text or symbols. |
| 10. | True | False | Placards must be visible on all 4 side of freight containers or transport vehicles. |
| 11. | True | False | Shipping Papers must include the following information:  Proper Shipping Name, Hazard Class or Division, Identification Number |
| 12. | True | False | If a shipment contains both Hazardous and Non-Hazardous materials the Hazardous material must be listed first or highlighted on the shipping papers. |
| 13. | True | False | The Material Safety Data Sheet (MSDS) does not contain emergency phone numbers and response information. |
| 14. | True | False | It is not necessary to list an emergency response telephone on shipping papers. |
| 15. | True | False | The person who signs the shipping paper certifies that the information is complete and accurate and that the materials have been prepared for transportation. |
| 16. | True | False | Incompatible Hazardous materials may not be loaded or stored next to each other. |
| 17. | True | False | Hazardous materials must be locked and braced during transportation |
| 18. | True | False | The Identification Numbers for Sulfuric Acid used at Giles is 1830 |
| 19. | True | False | You are permitted to accept packages of hazardous materials with damaged labels as long as you can read the full product name |
| 20. | True | False | Verbal notification to the DOT is required if a Hazardous material incident causes an evacuation of the general public for an hour or more. |